<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-PM11</Model>
<System>ORDER NO. MD0102023C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0500000000x</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=May year=2001>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-PM11</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>5 Handling Precautions For Traverse Deck</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0400000000x
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0600000000x
</nmlist>
</nameloc>
</Para>
<Para>The laser diode in the traverse deck (optical pickup) may break down due to potential difference caused by static electricity of clothes or human body.</Para>
<Para>So, be careful of electrostatic breakdown during repair of the traverse deck (optical pickup).</Para>
<Para><randlist prefix=unorder><item><Para><emphasis>Handling of traverse deck (optical pickup)</emphasis>
</Para>
</item>
</randlist>
</Para>
<Para><seqlist><item><Para>Do not subject the traverse deck (optical pickup) to static electricity as it is extremely sensitive to electrical shock.</Para>
</item>
<item><Para>The short land between the No.4(LD) and No.5(GND) pins on the flexible board (FFC) is shorted with a solder build-up to prevent damage to the laser diode.To connect to the PC board, be sure to open by removing the solder build-up, and finishthe work quickly.</Para>
</item>
<item><Para>Take care not to apply excessive stress to the flexible board (FFC).</Para>
</item>
<item><Para>Do not turn the variable resistor (laser power adjustment). It has already been adjusted.</Para>
</item>
</seqlist>
</Para>
<Figure><graphic boardno="graphic8" reprowid="90.847mm" reprodep="78.486mm" location="internal"></Figure>
<Para><randlist prefix=unorder><item><Para><emphasis>Grounding for electrostatic breakdown prevention</emphasis>
</Para>
<Para><seqlist><item><Para>Human body grounding</Para>
<Para>Use the anti-static wrist strap to discharge the static electricity from your body.</Para>
</item>
<item><Para>Work table grounding</Para>
<Para>Put a conductive material (sheet) or steel sheet on the area where the traverse deck (optical pickup) is placed, and ground the sheet.</Para>
</item>
</seqlist>
</Para>
<Para></Para>
<Para><emphasis>Caution :</emphasis></Para>
<Para>The static electricity of your clothes will not be grounded through the wrist strap. So, take care not to let your clothes touch the traverse deck (optical pickup).</Para>
<Para><emphasis>Caution when Replacing the Traverse Deck :</emphasis></Para>
<Para>The traverse deck has a short point shorted with solder to protect the laer diode against electroststics breakdown. Be sure to remove the solder from the short point before making connections.</Para>
<Figure><graphic boardno="graphic9" reprowid="91.271mm" reprodep="41.402mm" location="internal"></Figure>
</item>
</randlist>
</Para>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0400000000x
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0600000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
