<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-PM11</Model>
<System>ORDER NO. MD0102023C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1304000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=May year=2001>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-PM11</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>13.4 IC600 (M38258MCM084) System Microprocessor</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1303000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1400000000x
</nmlist>
</nameloc>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.640in"><colspec colnum="2" colname="2" colwidth="0.734in"><colspec colnum="3" colname="3" colwidth="0.535in"><colspec colnum="4" colname="4" colwidth="1.492in"><thead><row rowsep="1"><entry colname="1" align="center"><Para><emphasis>No.</emphasis>
</Para>
</entry>
<entry colname="2" align="center"><Para><emphasis>Mark</emphasis>
</Para>
</entry>
<entry colname="3" align="center"><Para><emphasis>I&sol;O</emphasis>
</Para>
</entry>
<entry colname="4" align="center"><Para><emphasis>Function</emphasis>
</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>VL1</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>LCD Bias</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>3</Para>
</entry>
<entry colname="2" align="justify"><Para>REGION_IN</Para>
</entry>
<entry colname="3" align="justify"><Para>A-D I</Para>
</entry>
<entry colname="4" align="justify"><Para>Region and function setting</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>DECK_AD1</Para>
</entry>
<entry colname="3" align="justify"><Para>A-D I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tape mecha condition input (HALF&sol;MODE&sol;RECIN_R/&sol;RECIN_F)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>DECK_AD2</Para>
</entry>
<entry colname="3" align="justify"><Para>A-D I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tape mecha condition input (TPS, PHOTO)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>6</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY 1</Para>
</entry>
<entry colname="3" align="justify"><Para>A-D I</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 1 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>7</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY 2</Para>
</entry>
<entry colname="3" align="justify"><Para>A-D I</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 2 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>8</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY 3</Para>
</entry>
<entry colname="3" align="justify"><Para>A-D I</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 3 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>9</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_AD1</Para>
</entry>
<entry colname="3" align="justify"><Para>A-D I</Para>
</entry>
<entry colname="4" align="justify"><Para>CHNGR SW A-D DETECTION INPUT 1</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>10</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_AD2</Para>
</entry>
<entry colname="3" align="justify"><Para>A-D I</Para>
</entry>
<entry colname="4" align="justify"><Para>CHNGR SW A-D DETECTION INPUT 2</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>11</Para>
</entry>
<entry colname="2" align="justify"><Para>EECS</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM chip select output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>12</Para>
</entry>
<entry colname="2" align="justify"><Para>EEDAT/&sol;ASP_DATA</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM data input &sol; ASP control data output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>13</Para>
</entry>
<entry colname="2" align="justify"><Para>EECLK/&sol;ASP_CLK</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>EECLKoutput &sol; ASP control clock output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>14</Para>
</entry>
<entry colname="2" align="justify"><Para>ASP/_LATCH</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>ASP control latch output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>15</Para>
</entry>
<entry colname="2" align="justify"><Para>MLD/&sol;PLLCE</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD command load output&sol;Tuner PLL chip enable</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>16</Para>
</entry>
<entry colname="2" align="justify"><Para>MDATA/&sol;PLLDA</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD command data output&sol;Tuner PLL chip output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>17</Para>
</entry>
<entry colname="2" align="justify"><Para>MCLK/&sol;PLLCLK</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD command data output&sol;Tuner PLL chip output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>18</Para>
</entry>
<entry colname="2" align="justify"><Para>BLKCK</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD Block clock input (Inverted)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>19</Para>
</entry>
<entry colname="2" align="justify"><Para>STATUS</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD Signal Processor status input (INV)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>20</Para>
</entry>
<entry colname="2" align="justify"><Para>SQCK&sol;ST/&sol;DO</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Subcode clock output &sol; Tuner IF data &sol; Stereo Input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>21</Para>
</entry>
<entry colname="2" align="justify"><Para>SD</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner Signal detect input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>22</Para>
</entry>
<entry colname="2" align="justify"><Para>SUBQ</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD Subcode data input (INV)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>23</Para>
</entry>
<entry colname="2" align="justify"><Para>RMT</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Remote control input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>24</Para>
</entry>
<entry colname="2" align="justify"><Para>SYNC</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>AC failure detect input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>25</Para>
</entry>
<entry colname="2" align="justify"><Para>PLED</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Primary relay control</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>26</Para>
</entry>
<entry colname="2" align="justify"><Para>PCONT</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Secondary relay control output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>27</Para>
</entry>
<entry colname="2" align="justify"><Para>REST_SW</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD limit SW input for the most inner point</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>28</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>No connection</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>29</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>No connection</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>30</Para>
</entry>
<entry colname="2" align="justify"><Para>SER_CLK</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Serial output clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>31</Para>
</entry>
<entry colname="2" align="justify"><Para>SER_DATA</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Serial output data</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>32</Para>
</entry>
<entry colname="2" align="justify"><Para>CDRST</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD reset output control</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>33</Para>
</entry>
<entry colname="2" align="justify"><Para>DCDET 1</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>DC Detect input 1</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>34</Para>
</entry>
<entry colname="2" align="justify"><Para>DCDET 2</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>DC Detect input 2</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>35</Para>
</entry>
<entry colname="2" align="justify"><Para>RESET</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>RESET input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>36</Para>
</entry>
<entry colname="2" align="justify"><Para>XCIN</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>32.768 kHz sub clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>37</Para>
</entry>
<entry colname="2" align="justify"><Para>XCOUT</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>32.768 kHz sub clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>38</Para>
</entry>
<entry colname="2" align="justify"><Para>XIN</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>8.0 MHz main clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>39</Para>
</entry>
<entry colname="2" align="justify"><Para>XOUT</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>8.0 MHz main clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>40</Para>
</entry>
<entry colname="2" align="justify"><Para>VSS</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Ground (0V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>41</Para>
</entry>
<entry colname="2" align="justify"><Para>MBP1</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>MPU beat proof output 1</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>42</Para>
</entry>
<entry colname="2" align="justify"><Para>MBP 2</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>MPU beat proof output 2</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>43</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_SW 2</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD changer switch 2 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>44</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_SW 1</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD changer switch 1 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>45</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_PLGR</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Changer plunger output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>46</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_HALF</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Changer half drive mode</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>47</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_CCW</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Changer motor CCW output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>48</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_CW</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Changer motor CW output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>49</Para>
</entry>
<entry colname="2" align="justify"><Para>VJOG_B</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Main volume jog input B</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>50</Para>
</entry>
<entry colname="2" align="justify"><Para>VJOG_A</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Main volume jog input A</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>51-55</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>No connection</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>56-90</Para>
</entry>
<entry colname="2" align="justify"><Para>SEG34/-SEG0</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Segment drive output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>91</Para>
</entry>
<entry colname="2" align="justify"><Para>VCC</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Power supply (&plus;5V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>92</Para>
</entry>
<entry colname="2" align="justify"><Para>VREF</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Reference for A-D</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>93</Para>
</entry>
<entry colname="2" align="justify"><Para>AVSS</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Analog ground (0V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>94</Para>
</entry>
<entry colname="2" align="justify"><Para>COM3</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>LCD common 3 output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>95</Para>
</entry>
<entry colname="2" align="justify"><Para>COM2</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>LCD common 2 output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>96</Para>
</entry>
<entry colname="2" align="justify"><Para>COM1</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>LCD common 1 output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>97</Para>
</entry>
<entry colname="2" align="justify"><Para>COM0</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>LCD common 0 output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>98</Para>
</entry>
<entry colname="2" align="justify"><Para>VL3</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>LCD Bias</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>99</Para>
</entry>
<entry colname="2" align="justify"><Para>VL2</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>LCD Bias</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>100</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>OPEN</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1303000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1400000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
