<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-PM11</Model>
<System>ORDER NO. MD0102023C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0802000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=May year=2001>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-PM11</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>8.2 Main Component Replacement Procedures</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0801000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0803000000
</nmlist>
</nameloc>
</Para>
<Para><emphasis>1. Replacement of the Traverse Deck</emphasis>
</Para>
<Para><emphasis>Step 1</emphasis>
Follow the procedures in &lsquo;Disassembly of the Traverse Unit&rsquo; ( Step 1 - Step 4 )</Para>
<Figure><graphic boardno="graphic18" reprowid="79.248mm" reprodep="54.695mm" location="internal"></Figure>
<Figure><graphic boardno="graphic19" reprowid="47.096mm" reprodep="55.386mm" location="internal"></Figure>
<Para><emphasis>Step 3</emphasis>
Desolder the 4 legs of the 2 motors and pull out the Servo P.C.B.</Para>
<Para><emphasis>Step 4</emphasis>
Widen the 3 bosses with a flat screwdriver and pull out the 3 pins. Then remove the Traverse Deck.</Para>
<Figure><graphic boardno="graphic20" reprowid="79.248mm" reprodep="121.920mm" location="internal"></Figure>
<Para><emphasis>Step 5</emphasis>
Remove the flexible cable CN 701.</Para>
<Para><randlist prefix=unorder><item><Para>Removal of the flexible cable. Push the top of the connector in the direction of the arrow 1, and then pull out the flexible cable in the direction of the arrow 2.</Para>
</item>
</randlist>
</Para>
<Para><emphasis>Note:</emphasis>
</Para>
<Para>Insert a short pin into the flexible cable for traverse unit.</Para>
<Para><randlist prefix=unorder><item><Para><emphasis>Installation of the CD servo P.C.B. after replacement</emphasis>
</Para>
</item>
</randlist>
</Para>
<Para><emphasis>Step 1</emphasis>
Connect the FFC board.</Para>
<Para><emphasis>Step 2</emphasis>
Install the CD servo P.C.B. in the traverse deck assembly.</Para>
<Figure><graphic boardno="graphic21" reprowid="85.937mm" reprodep="87.165mm" location="internal"></Figure>
<Para><emphasis>Note:</emphasis>
</Para>
<Para>Before installing the CD servo P.C.B., move the optical pickup towards the outer edge from the marking (black triangle). [Otherwise, the reset detect switch (S701) mounted on the CD servo P.C.B. may be damaged.]</Para>
<Figure><graphic boardno="graphic22" reprowid="87.389mm" reprodep="43.545mm" location="internal"></Figure>
<Para><emphasis>2. Replacement of the Power Amplifier IC</emphasis>
</Para>
<Para><emphasis>Step 1</emphasis>
Follow the procedures in &lsquo;Checking Procedure for each major P.C.B.&rsquo; ( Step 1 - Step 6 ).</Para>
<Figure><graphic boardno="graphic16" reprowid="71.797mm" reprodep="73.491mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
Remove the wires at CN302, CN303 and CN304 and pull out the Main P.C.B.</Para>
<Figure><graphic boardno="graphic15" reprowid="77.893mm" reprodep="102.108mm" location="internal"></Figure>
<Para><emphasis>Step 5</emphasis>
Remove 4 screws fixed to the Power Amplifier IC.</Para>
<Figure><graphic boardno="graphic23" reprowid="79.587mm" reprodep="69.765mm" location="internal"></Figure>
<Para><emphasis>Step6</emphasis>
Unsolder the terminals of Power Amp IC and replace the respective component.</Para>
<Figure><graphic boardno="graphic24" reprowid="77.385mm" reprodep="100.923mm" location="internal"></Figure>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0801000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0803000000
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
