10K

4.7K

NON-POLARIZED

15 UF

                                                                                                             5

                                                                                                             6
                                                                                                                       7

                                                                                                                      U3B

                                                                                                                 TL022C

                                                                                 10 UF
                                                                                                22K

                                                                      56 UF
                                    47 UF

                                            Q1
                                           J111

                         1N4001

                 22K

                                               Q2
                                               2N5089

                                                 100K
                                                             100K

                                                             10K

                                                                                              22K

220K

                                                                                                                180K
                                                                                                        2K

                                                                                                                SPEED
                                                                                                                500K

  3

  2
 1

8

4 U3A

TL022C

VCC

WIDTH

100K

220K 1N4148

100K

4.7K

1N4148

5K

150K

10UF
10K

100K

                                                                                                                 100K
                                                                              P1
                                                                              100K
                      0.0023
                               27K

                                330K

                        150K

            9Vdc

            JACK CREATES THE CIRCUIT
            GROUND.

            (*) PLUGGING INTO THE INPUT

           +

               VCC

                 470K

                  62K
                22K

IN (*)

       0.01

    10UF

                         3

                         2

                                  1

                             8

                             4

                                U1A

                                 TL022C

                                               10K

                                              47K

                           VCC

                                                     47K

                                            0.001 120PF 4.7K

                                                                                    470K

                                                                          0.047

                                                                                                                1

                                                                                                                2

                                                                                                                3

                                                                                                                4 5

6

7

8

                                                                                                                  MN3007
1

2

3

4

MN3101

5

6

7

8

1K
33K

Q3
2N4125

Q4

2N4124

25 PF

0.005

 3

 2
  1

8

4 U2A

TL022C

                                                                                                     100K

                                                                       1N4148

                                                       1N4148
                          33K 0.022

                                  62K
         REGENERATION
                         500K

             100K

                     1K

              1 UF

OUT

                                               47K

                                47K

                                0.0063

                             10K

                                     5

                                     6

                            7

                                    U2B

                                    TL022C

                                                                                             Q5
                                                                                             J113

                                                                                                   1M
                                                                                      0.047

                                                                                     1N4148

                                                                                                                       1SP

                                                                                                                    2 1DP

                                                                                                                    1 1A

 3
                                                                                                                       1DN

                                                                                                                    5 1SN

                                                                                                                    4

                                                                                                                       VDD

                                                                                                                   14 2DP

                                                                                                                   13 2A

 6

                                                                                                                       2DN

                                                                                                                    8 VSS

                                                                                                                    7

                                                                                                                       3SP

                                                                                                                   11 3A

10
                                                                                                                       3Y

                                                                                                                   12 3SN

                                                                                                                    9

                                                                                                                       U6

                                                                                                                       CD4007

0.047

1M VCC

33K 33K

0.001

120PF

33K

MN3007 AUDIO SIGNAL DELAY, 1024 STAGE LOW NOISE BBD
 (5.12-51.2 msec delay)

PARTS DESCRIPTION:

CD4007 DUAL COMPLEMENTARY PAIR WITH INVERTER; (RCA)

MN3101 CLOCK GENERATOR FOR BUCKET BRIGADE DEVICE /BBD

TL022C LOW POWER DUAL OPAMP; (TEXAS INSTRUMENTS)

                                                                                                               1M

                                                                                                    100K

                                                                                            10K

                                                                                               Q6

                                                                                            2N5089

                              120PF

                                    5

                                    6

                          7

                                   U1B

                             TL022C

                   4.7K

             1 UF

OUT

            100K

                                47K

                              120PF

                                                                                                    10K

                                                                                          A COMMON POINT (OR JUNCTION) IS ILLUSTRATED BY >>
                                                                                          WHEN THIS IS NOT SEEN, WIRES WHICH CROSS OVER EACH
                                                                                          OTHER ON THIS SCHEMATIC ARE "NOT" CONNECTED.

                                                                                                               0.047

MOMENTARY SWITCH
USED TO ENGAGE EFFECT

MN3101/MN3007 MANF. PANASONIC; THESE ARE EQUIVALENT
TO ECG1639/ECG1641 RESPECTFULLY.

Date:  November 20, 1994 Sheet     1 of     1

Size Document Number REV

B DRAWN BY: FABIAN P. HARTERY 1

Title
DOD FX75 FLANGER (10-15-84)