# RS422 serial information |
Web | www.lammertbies.nl

| Quick links
• | RS-232 specs
• | RS-423 information
• | RS-485 information
• | The serial UART
• | RS-232 cables
• | Unitronics RJ11
• | PLC cables
• | Modbus interface
• | USB interface
• | Software download
| Save this page to del.icio.us On these pages Introduction to RS422 Differential balanced signals with RS422 Electrical characteristics of RS422 Network topology with RS422 RS422 support forum New # Introduction to RS422 Serial communication methods to transfer information between equipment have been defined by standards for nearly half a century. The oldest and best known standard is RS232, a standard which defines the communication between DTE, data terminal equipment, and DCE, data communication equipment. The relatively short distances and low speed the RS232 serial interface can handle demanded for newer standards like RS422, RS423 and RS485. In this document, I will focus on the RS422 interface for serial balanced differential communications. ## Differential balanced signals with RS422 Serial, balanced and differential are the keywords for the RS422 interface standard. Serial means, that the information is sent bit by bit on a single transmission line, just like with RS232. Balanced differential is what makes RS422 different from RS232. On RS232 interfaces, the signals are send on lines which share a common zero. With RS422, each signal line consists of two wires, preferably twisted to reduce noise. The voltage-difference between the two lines is an indication of the signal value, rather than the voltage-level. Looking at voltage differences with RS422 rather than levels eliminates a lot of noice induced by external sources and allows for higher data rates and cable lengths compated to RS232. You can see the differences in speed and cable length between RS422 and other commonly used serial interface standards like RS232, RS423 and RS485 in the interface comparison table. Twisting the lines helps to reduce the noise. The noise currents induced by an external source are reversed in every twist. Instead of amplifying each other as in a straight line, the reversed noice currents reduce each others influence. The figure explains this in more detail. Noise in straight and twisted pair cables ## Network topology with RS422 There are more differences between RS422 and RS232 than the maximum data speed and cable length. RS232 was specifically defined as an interface between computers, printers and terminals with modems. The modem would translate the communication signals to protocol usable for long distance communication, where long distance could also mean a device on the other side of the control room or building. RS422 allows the direct connection of intelligent devices, without the need of modems. Furthermore, where the RS232 linedriver is only designed to serve one receiver, a RS422 linedriver can serve upto ten receivers in parallel. This allows one central control unit to send commands in parallel to upto ten slave devices. Unfortunately, those slave devices cannot send information back over a shared interface line. RS422 allows a multi-drop network topology, rather than a multi-point network where all nodes are considered equal and every node has send and receive capabilities over the same line. If you need to build a multi-point communication network rather than multi-drop, RS485 is the right choice with a maximum of 32 parallel send and 32 receive units parallel on one communication channel.
Leftover nuts never match leftover bolts. THIRD WORKSHOP PRINCIPLE

General cables
General cables
Null modem cables
Null modem cables
Printer cables
Printer cables
Spy / monitor cables
Spy / monitor cables
DEC MMJ cables
DEC MMJ cables
Yost RS232 to RJ45
Yost RS232 to RJ45
RJ-45, RJ11, etc.
RJ-45, RJ11, etc.
DEC MMJ cables
DEC MMJ cables
Yost RS232 to RJ45
Yost RS232 to RJ45
Unitronics RJ11
Unitronics RJ11
RS-232 specifications
RS-232 specifications
RS-422 specifications
RS-422 specifications
RS-423 specifications
RS-423 specifications
RS-485 specifications
RS-485 specifications
UART information
UART information
I/O ports and IRQ's
I/O ports and IRQ's
RS232 flow control
RS232 flow control
Which RS232 null modem?
Which RS232 null modem?
USB specifications
USB specifications
USB to RS-232 converters
USB to RS-232 converters
Siemens
Siemens
Omron
Omron
Mitsubishi
Mitsubishi
Unitronics
Unitronics
Other brands
Other brands
RS-232
RS-232
»
PLC
PLC
»
Modular
Modular
»
Parallel
Parallel
VGA monitor
VGA monitor
Modbus protocol
Modbus protocol
I2C bus
I2C bus
RS232, 422, 423, 485
RS232, 422, 423, 485
»
USB
USB
»
Bus systems
Bus systems
»
Hayes AT commands
Hayes AT commands
On-line CRC calculation
On-line CRC calculation
ASCII character set
ASCII character set
Schmitt trigger inputs
Schmitt trigger inputs
Cable information
Cable information
»
General information
General information
»
Software downloads
Software downloads
Webshop
Webshop
Who am I?
Who am I?
Hobbies
Hobbies
My work
My work
Travel
Travel
My friends
My friends
Contact
Contact