Monitor Make | Monitor Model | Problem | Solution
--- | --- | --- | ---
DELL | V1428U | BRIGHTNESS CONTROL INOP, GETS TOO BRIGHT & SHUTS OFF | R439 2M-1/2W OPEN
DELL | V1428U | PIX TEARS UP THE MIDDLE WHEN HOT, TAPPING NEAR D415 AFFECTS | D415 HEATSINK TOUCHING R467 & BURNED THRU INSULATOR, REPL INSULATOR.
DELL | V1428U | POWER SUPPLY IN SHUTDOWN, LIGHT FLASHES ON & OFF | Q403 2SC3886 (ECG2324), C428 1UF/50V, C808 330UF/250V
DELL | V1428U | WIDTH NARROW, WIDTH CONTROL NO EFFECT, HORZ SMALL | Q411 2SC2073 (ECG375), R464 1-11/2W,Q403 2SC4742 (ECG2302)
DELL | V1428U | WIDTH TOO WIDE AFTER WARMUP, UNIT DRAWS 80-95 WATTS | C818 47UF/160, C424 33UF/160V, R428 10K-1/2W CAPS HAD BAD ESR
DELL | DL-1462NI | NO POWER ON | REPLACE D109 1N5404
DELL | VC-7N | SHUT DOWN AFTER DEGAUSS CYCLE | REPLACE FLYBACK FBA06A12H1BX
DELL | VC-7N | NO VIDEO | IC202, IC203 CHECK
DELL | VC-7N | NO HV | CHECK SOLDER ON Q603 AND FBT
DELL | VC-7N | SHUTS DOWN AFTER 10 SEC. | DEAD FAN…REPLACE
DELL | TFS-6705KW | SHUTS DOWN AFTER 10 SEC. | DEAD FAN…REPLACE
DELL | VI1439U | IMAGE FADES | LOSING 12V…CHECK R611, R601, IC602 ECG966
DELL | HSU-TRLCX | IMAGE FADES | LOSING 12V…CHECK R611, R601, IC602 ECG966
DELL | 17FS-N | NO GREEN…WON'T DEGAUSS | IC201 AND CHECK FAN
DELL | TFS-6705 | NO GREEN…WON'T DEGAUSS | IC201 AND CHECK FAN
DELL | MOST MODELS | SHUT DOWN AFTER 10 SEC | CHECK FAN…WILL SHUT UNIT DOWN IF INOP
DELL | VC-1 | IMAGE IS JUMPY/JITTERS | CHECK ALL P/S CAPS FOR PROPER VALUES
DELL | CA-6 | IMAGE IS JUMPY/JITTERS | CHECK ALL P/S CAPS FOR PROPER VALUES
DELL | VC-2 | DEAD | Q901 ECG129P, IC901 STR53041, C924 1000/25V, D905 ECG558
DELL | VC-2 | SQUEAL AFTER WARM UP | CHECK ALL P/S CAPS
DELL | VC-10CEN | NO BLUE | Q812 ECG32…REPLACE
DELL | VI428U | B+ TOO HIGH, HV SHUTS DOWN | ALING TP1 TO EQUAL 91-93VDC FREE RUNNING
DELL | VI428U | BRIGHT RASTER, VARIOUS COLORS | R439
DELL | VI428U | CUTS OUT OR FAILS TO START | CHECK ALL Q801, C828, R827, R825
DELL | VC5 | FULL BRIGHTNESS…CAN'T ADJ | C417 10/250V
DELL | P1528U | BLUE SCREEN | VIDEO IC BAD LM1203N
DELL | P1528U | GREEN ONLY | VIDEO IC BAD LM1230N
DELL | VI428U | VIDEO TOO DARK | CHECK ALL GROUNDS ON CRT PCB
DELL | VI428U | WENT COMPLETELY BLACK | C828 AND SOLDER UP
DELL | 17FS-N | SHUTS DOWN AFTER POWER UP | REPLACE FAN FBA-06A12H1B1
DELL | 17FS-N | DEAD | SHORTED 160V LINE…REPLACE Q603
DELL | VC-5 | NO VIDEO | CHECK ALL C210, 240, 270, 208, 238, 268, 209, 239, 269, VIDEO IC M51387
DELL | VC-5 | SCREEN TOO BRIGHT | C417 10/250V
DELL | P1428U | HORIZONTAL LINES, HORIZONTAL FREQ OFF | BAD IC501 PN: KA2135 OR ECG7045

***** End of monitor database search *****