From - Wed Jul 15 16:33:15 1998
Return-Path: <monitor-repair-return-150-dmfraser=wave.home.com@makelist.com>
Received: from h1.mail.home.com ([24.0.0.50]) by ha1.rdc1.bc.wave.home.com
          (Post.Office MTA v3.5 release 217 ID# 1-1U40000L0S0V35)
          with ESMTP id com for <dmfraser@mail.surrey1.bc.wave.home.com>;
          Wed, 15 Jul 1998 11:56:02 -0700
Received: from mx2.home.com (mx2.home.com [24.2.0.31])
	by h1.mail.home.com (8.9.0/8.9.0) with ESMTP id LAA04591
	for <dmfraser@wave.home.com>; Wed, 15 Jul 1998 11:56:01 -0700 (PDT)
Received: from findmail.com (vault.findmail.com [209.185.96.136])
	by mx2.home.com (8.8.5/8.8.5-AtHome) with SMTP id LAA15092
	for <dmfraser@wave.home.com>; Wed, 15 Jul 1998 11:55:58 -0700 (PDT)
Received: (qmail 10007 invoked by uid 505); 15 Jul 1998 16:51:35 -0000
Mailing-List: contact monitor-repair-help@makelist.com; run by ezmlm
Precedence: list
X-URL: http://www.findmail.com/list/monitor-repair/
X-Mailing-List: monitor-repair@makelist.com
Reply-To: monitor-repair@makelist.com
Delivered-To: mailing list monitor-repair@makelist.com
Received: (qmail 9298 invoked by uid 7770); 15 Jul 1998 16:51:03 -0000
Received: from www.mauigateway.com (205.166.249.5)
  by vault.findmail.com with SMTP; 15 Jul 1998 16:51:03 -0000
Received: from seaqmaui.com (mgate-223.mauigateway.com [205.166.249.223]) by www.mauigateway.com (8.8.5/8.6.12) with ESMTP id GAA13930 for <monitor-repair@makelist.com>; Wed, 15 Jul 1998 06:50:06 -1000 (HST)
Message-ID: <35ACDDDE.4636C78D@seaqmaui.com>
Date: Wed, 15 Jul 1998 06:50:38 -1000
From: terry <terry@seaqmaui.com>
X-Mailer: Mozilla 4.04 [en] (Win95; I)
MIME-Version: 1.0
To: monitor-repair@makelist.com
Subject: Re: [monitor-repair] Pin problem on Mitsubishi AUM-1381
References: <35ACC1DB.97E42887@senecac.on.ca>
Content-Type: multipart/mixed; boundary="------------6132B1A1EE8AC3CB5ACE2F92"
X-Mozilla-Status: 8011

This is a multi-part message in MIME format.
--------------6132B1A1EE8AC3CB5ACE2F92
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

shhhhhhhhhhhhhhh
--------------6132B1A1EE8AC3CB5ACE2F92
Content-Type: text/html; charset=iso-8859-1; name="monitorback1.html"
Content-Transfer-Encoding: quoted-printable
Content-Disposition: inline; filename="monitorback1.html"
Content-Base: "file:///H|/mits/monitorback1.html"

<!-- monitorback1.html -->

<html>

<body>

<font face=3D"arial,helv" size=3D3>

<center><h3>Retrieving monitor data by make/brand - please standby...</h3=
><br>

<b>Displaying search results for: <font color=3D"#ff0000">

mitsubishi<p>

<TABLE BORDER>

<tr bgcolor=3D"#C2D4E8"><th><font face=3D"arial,helv" size=3D2 color=3D"0=
00090">Monitor Make </th><th><font color=3D"000090" face=3D"arial" size=3D=
2> Monitor Model </th><th><font face=3D"arial,helv" size=3D2 color=3D"000=
090"> Problem </th><th><font face=3D"arial" size=3D2 color=3D"000090"> So=
lution </th></tr>

<tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td=
><font face=3Darial size=3D2>1381 </td><td><font face=3Darial size=3D2>IM=
AGE IS DULL=85FUZZY=85DIM </td><td><font face=3Darial size=3D2>TYPICALLY,=
 BAD CRT TUBE. </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial siz=
e=3D2>MITSUBISHI </td><td><font face=3Darial size=3D2>1381 </td><td><font=
 face=3Darial size=3D2>SQUEALING IN P/S AND/OR NO START </td><td><font fa=
ce=3Darial size=3D2>BAD C907(10/100V), C965 (10/200V) </td></tr><tr bgcol=
or=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font fa=
ce=3Darial size=3D2>1381 </td><td><font face=3Darial size=3D2>PCC PROBLEM=
 </td><td><font face=3Darial size=3D2>C5AB (220/16V NEAR TOP OF CHASSIS) =
BAD </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSU=
BISHI </td><td><font face=3Darial size=3D2>1381 </td><td><font face=3Dari=
al size=3D2>BLOWS FUSE INTERMITTENTLY </td><td><font face=3Darial size=3D=
2>REPLACE DEGAUSS POSISTOR, USE SLOW BLOW FUSE </td></tr><tr bgcolor=3D#E=
7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Dar=
ial size=3D2>1429 </td><td><font face=3Darial size=3D2>INCOMPLETE IMAGE I=
N GRAPHICS MODES </td><td><font face=3Darial size=3D2>CHECK Q203 (ECG289A=
) </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBI=
SHI </td><td><font face=3Darial size=3D2>1429 </td><td><font face=3Darial=
 size=3D2>VIDEO IC CONSTANT FAILURE </td><td><font face=3Darial size=3D2>=
CRT POSSIBLY ARCING INSIDE WHICH KILLS VIDEO IC </td></tr><tr bgcolor=3D#=
E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Da=
rial size=3D2>1429 </td><td><font face=3Darial size=3D2>BRIGHTNESS AND CO=
NTRAST NON FUNCTIONAL </td><td><font face=3Darial size=3D2>CHECK R228 10K=
 AND Q204 ECG289A=85ALSO CHECK IC201 </td></tr><tr bgcolor=3D#E7E8E8><td>=
<font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D=
2>1430 </td><td><font face=3Darial size=3D2>PICTURE IS WEAK=85WORSE WHEN =
WARM </td><td><font face=3Darial size=3D2>C958 (330/16V) BAD </td></tr><t=
r bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><=
font face=3Darial size=3D2>1430 </td><td><font face=3Darial size=3D2>DEAD=
 </td><td><font face=3Darial size=3D2>REPLACE/CHECK ON/OFF SWITCH </td></=
tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td>=
<td><font face=3Darial size=3D2>1430 </td><td><font face=3Darial size=3D2=
>NO HV=85FUSE F951 BLOWN </td><td><font face=3Darial size=3D2>C556, D925,=
 AND FUSE PICO 1A=85REPLACE </td></tr><tr bgcolor=3D#E7E8E8><td><font fac=
e=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D2>1430 <=
/td><td><font face=3Darial size=3D2>LOSS OF POWER SUPPLY AND HV AFTER POW=
ER ON </td><td><font face=3Darial size=3D2>C407, C412, IC401, IC402, C515=
, C529 </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MI=
TSUBISHI </td><td><font face=3Darial size=3D2>AUM-1381 </td><td><font fac=
e=3Darial size=3D2>DEAD </td><td><font face=3Darial size=3D2>REPLACE POSI=
STOR, 4A SLOW BLOW </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial=
 size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D2>AUM-1381 </td><=
td><font face=3Darial size=3D2>DIM=85SLOW WARM UP </td><td><font face=3Da=
rial size=3D2>IN PS: C5AC, C580, C5A5, C577, R573 1.5K/3 </td></tr><tr bg=
color=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font=
 face=3Darial size=3D2>C-5470NS </td><td><font face=3Darial size=3D2>DEAD=
 </td><td><font face=3Darial size=3D2>IN PS: C914, C911, C923, PC901, PC9=
02 </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUB=
ISHI </td><td><font face=3Darial size=3D2>C-5470NS </td><td><font face=3D=
arial size=3D2>DEAD </td><td><font face=3Darial size=3D2>IN PS: C914, C91=
1, C923, PC901, PC902 ECG3041 </td></tr><tr bgcolor=3D#E7E8E8><td><font f=
ace=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D2>FW-6=
405 </td><td><font face=3Darial size=3D2>CAN NOT CENTER UP THE VERTICAL <=
/td><td><font face=3Darial size=3D2>C413 </td></tr><tr bgcolor=3D#E7E8E8>=
<td><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial si=
ze=3D2>FW-6405 </td><td><font face=3Darial size=3D2>HORIZOTAL SHIMMY </td=
><td><font face=3Darial size=3D2>C915 </td></tr><tr bgcolor=3D#E7E8E8><td=
><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D=
2>FW-6405ATK </td><td><font face=3Darial size=3D2>YELLOW AND RED STREAKS=85=
NO BLUE </td><td><font face=3Darial size=3D2>CHECK SOLDER ON MAIN BOARD <=
/td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI=
 </td><td><font face=3Darial size=3D2>HA3905ADK </td><td><font face=3Dari=
al size=3D2>EXCESS HV SHUTDOWN </td><td><font face=3Darial size=3D2>SHORT=
ED Q951 IN P/S (ALSO CAUSED FLYBACK/HORIZ TO SHORT) </td></tr><tr bgcolor=
=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=
=3Darial size=3D2>HC-3905 </td><td><font face=3Darial size=3D2>HORIZONTAL=
 ROLL </td><td><font face=3Darial size=3D2>IC503, Q502 </td></tr><tr bgco=
lor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font f=
ace=3Darial size=3D2>HJ-6905ATK </td><td><font face=3Darial size=3D2>DEAD=
 </td><td><font face=3Darial size=3D2>Q510, C908, C909, Q901, R908 3.9K/5=
W </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBI=
SHI </td><td><font face=3Darial size=3D2>HL-6605 </td><td><font face=3Dar=
ial size=3D2>DEAD </td><td><font face=3Darial size=3D2>Q951, Q411, Q507, =
D524, D525 </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D=
2>MITSUBISHI </td><td><font face=3Darial size=3D2>HL-6675 </td><td><font =
face=3Darial size=3D2>HIGH PITCHED SQUEAL </td><td><font face=3Darial siz=
e=3D2>Q507, Q411, Q951, D524, D525 </td></tr><tr bgcolor=3D#E7E8E8><td><f=
ont face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D2=
>HL-6905TK </td><td><font face=3Darial size=3D2>DIES AFTER ABOUT 1 HOUR <=
/td><td><font face=3Darial size=3D2>COLD SOLDER ON DEFLECTION BOARD </td>=
</tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </t=
d><td><font face=3Darial size=3D2>HL6605 </td><td><font face=3Darial size=
=3D2>P/S SHORTED=85LOSS OF HORIZONTAL DEFLECTION </td><td><font face=3Dar=
ial size=3D2>CHECK Q507, Q951, Q411, R441, R541, R542, D524, D525, C563 <=
/td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI=
 </td><td><font face=3Darial size=3D2>HL6615 </td><td><font face=3Darial =
size=3D2>P/S SHORTED=85LOSS OF HORIZONTAL DEFLECTION </td><td><font face=3D=
arial size=3D2>CHECK Q507, Q951, Q411, R441, R541, R542, D524, D525, C563=
 </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBIS=
HI </td><td><font face=3Darial size=3D2>HL6905 </td><td><font face=3Daria=
l size=3D2>P/S SHORTED=85LOSS OF HORIZONTAL DEFLECTION </td><td><font fac=
e=3Darial size=3D2>CHECK Q507, Q951, Q411, R441, R541, R542, D524, D525, =
C563 </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITS=
UBISHI </td><td><font face=3Darial size=3D2>HL6945ATK </td><td><font face=
=3Darial size=3D2>LOSS OF DEFLECTION/HV </td><td><font face=3Darial size=3D=
2>Q507, Q411, Q951, ADJUST VR501 FOR MIN VOLTAGE ON Q411 COLLECTOR </td><=
/tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td=
><td><font face=3Darial size=3D2>HL6945ATK </td><td><font face=3Darial si=
ze=3D2>VERTICAL FOLDOVER </td><td><font face=3Darial size=3D2>R444 8.2 BA=
D </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBI=
SHI </td><td><font face=3Darial size=3D2>HL6955 </td><td><font face=3Dari=
al size=3D2>SHUTS DOWN AFTER DEGAUSS CYCLE </td><td><font face=3Darial si=
ze=3D2>REPLACE FLYBACK FBA06A12L1BX </td></tr><tr bgcolor=3D#E7E8E8><td><=
font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D=
2>HL6955 </td><td><font face=3Darial size=3D2>VERTICAL FOLDOVER </td><td>=
<font face=3Darial size=3D2>R444 8.2 BAD </td></tr><tr bgcolor=3D#E7E8E8>=
<td><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial si=
ze=3D2>SC-1429C </td><td><font face=3Darial size=3D2>PURPLE COLOR AT PROM=
PT </td><td><font face=3Darial size=3D2>REPLACE CABLE 87-600 </td></tr><t=
r bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><=
font face=3Darial size=3D2>SD-4533 </td><td><font face=3Darial size=3D2>N=
O POWER </td><td><font face=3Darial size=3D2>CHECK R905 </td></tr><tr bgc=
olor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font =
face=3Darial size=3D2>SD-4533C </td><td><font face=3Darial size=3D2>VERTI=
CAL SIZE CONTROL CAUSES LOSS OF V HOLD </td><td><font face=3Darial size=3D=
2>ADJUST INSIDE V-HOLD </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Da=
rial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D2>SD-5500 </t=
d><td><font face=3Darial size=3D2>NO COLOR </td><td><font face=3Darial si=
ze=3D2>IC201, Q506, R201, R562 </td></tr><tr bgcolor=3D#E7E8E8><td><font =
face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D2>SD5=
500C </td><td><font face=3Darial size=3D2>COLOR BACKGROUND DISPLAY POOR <=
/td><td><font face=3Darial size=3D2>REPLACE IC201 WITH LM1203 </td></tr><=
tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td>=
<font face=3Darial size=3D2>SD5500C </td><td><font face=3Darial size=3D2>=
NO RED, GREEN, OR BLUE </td><td><font face=3Darial size=3D2>IC201 LM1203N=
 BAD, REPLACE R201 WITH 150 OHM 1/4W CARBON FILM </td></tr><tr bgcolor=3D=
#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3D=
arial size=3D2>SD5500C </td><td><font face=3Darial size=3D2>NO HV AND PRO=
BLEM WITH 75V LINE </td><td><font face=3Darial size=3D2>REPLACE D957, Q50=
6, Q957 </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>M=
ITSUBISHI </td><td><font face=3Darial size=3D2>SD5700C </td><td><font fac=
e=3Darial size=3D2>DEAD, NO INDICATOR </td><td><font face=3Darial size=3D=
2>F953 1.5A, F954 1A, D957 2.8V ZENER HZ3A3, Q951 2SB1095 </td></tr><tr b=
gcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><fon=
t face=3Darial size=3D2>TF7705 </td><td><font face=3Darial size=3D2>COLOR=
 BACKGROUND DISPLAY BAD </td><td><font face=3Darial size=3D2>CHECK IC201.=
=2E.RESOLDER VIDEO CABLES TO MAIN PCP </td></tr><tr bgcolor=3D#E7E8E8><td=
><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D=
2>TFS6705 </td><td><font face=3Darial size=3D2>SHUTS DOWN AFTER DEGAUSS C=
YCLE </td><td><font face=3Darial size=3D2>REPLACE FLYBACK FBA06A12L1BX </=
td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI =
</td><td><font face=3Darial size=3D2>TFS6705 </td><td><font face=3Darial =
size=3D2>NO VIDEO </td><td><font face=3Darial size=3D2>IC202, IC203 BAD <=
/td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI=
 </td><td><font face=3Darial size=3D2>TFS6705 </td><td><font face=3Darial=
 size=3D2>NO HIGH VOLTAGE </td><td><font face=3Darial size=3D2>CHECK SOLD=
ER ON Q603 AND FBT PINS </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3D=
arial size=3D2>MITSUBISHI </td><td><font face=3Darial size=3D2>XC-1410C <=
/td><td><font face=3Darial size=3D2>DEAD </td><td><font face=3Darial size=
=3D2>C407, IC401, IC402, C409, R521, D508, RG501 </td></tr><tr bgcolor=3D=
#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td><td><font face=3D=
arial size=3D2>XC-1429C </td><td><font face=3Darial size=3D2>NO BRIGHTNES=
S CONTROL </td><td><font face=3Darial size=3D2>R254, CR206, IC201, Q203 <=
/td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI=
 </td><td><font face=3Darial size=3D2>XC1410 </td><td><font face=3Darial =
size=3D2>DEAD </td><td><font face=3Darial size=3D2>C556, D925 BAD </td></=
tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D2>MITSUBISHI </td>=
<td><font face=3Darial size=3D2>XC3715C </td><td><font face=3Darial size=3D=
2>OSD ROLLS </td><td><font face=3Darial size=3D2>IC406 ...ALSO CHECK IC22=
2, 223, 226 </td></tr><tr bgcolor=3D#E7E8E8><td><font face=3Darial size=3D=
2>MITSUBISHI </td><td><font face=3Darial size=3D2>XC3725C </td><td><font =
face=3Darial size=3D2>DISPLAY DISTORTION NEAT TOP </td><td><font face=3Da=
rial size=3D2>R926 AND R947 REPLACE WITH 110 1/4WATT, R925 AND R948 REPLA=
CE WITH 33 1/4WAT </td></tr></TABLE><p>

<b><font face=3D"arial" color=3D"ff0000"> ***** End of monitor database s=
earch *****</b></font></font><p>

<font face=3D"arial,helv" size=3D2>

<img src=3D"/images/check.gif"> If you didn't find what you were looking =
for, try these suggestions:<ol>

<a href=3D"http://www.electronix.com/techsweb/forum.html">RepairWorld Rep=
air Forum</a> - Try posting your problem here for assistance.<br> <a href=
=3D"http://www.electronix.com/techsweb/techsinfo.html">Database Searching=
 Hints</a> - Check out these important hints and tips.<br>

<a href=3D"http://www.electronix.com/techsweb/techschat.html">TechsChat L=
ive</a> - Chat live on-line with other technician members.</ol><p>

<b>Use the back button on your browser to search again...<p></b>

<font size=3D1>Data Copyright (c) Electronix Corp. Fairborn, OH -  All ri=
ghts reserved.<br>

Select monitor repair tips are courtesy of KMR Technical Services, Inc. (=
james@kmrtech.com)

</font>

</body>

</html>
--------------6132B1A1EE8AC3CB5ACE2F92--



---- 
Read this list on the Web at http://www.makelist.com/list/monitor-repair/ 
To unsubscribe, email to monitor-repair-unsubscribe@makelist.com
To subscribe, email to monitor-repair-subscribe@makelist.com
--
Start a FREE E-Mail List at http://www.makelist.com !
