### Retrieving monitor data by make/brand - please standby...

Monitor Make | Monitor Model | Problem | Solution
--- | --- | --- | ---
NEC | JC1531VMA | DEAD | Q505 HPA100, Q510 IRF9610
NEC | JC1532VMA | PIX SHRUNK, PINCUSHION PROB | IC801 SYNC PROCESSOR HE6-0020
NEC | PVG-6431-2 | PIX INOP. MAKES CHIRPING SOUND | R321,R325,2SD1651
NEC | JC-1431VMA | POWER LIGHT BLINKING | Q403, Q405, IC403 HA17324
NEC | CM-14BA | POWER LIGHT BLINKING | Q403, Q405, IC403 HA17324
NEC | JC-1431VMA | VIDEO SHAKEY | TIGHTEN/REPLACE VERTICAL POT
NEC | JC-1401 | DEAD | IN PS: IC601, IC602, R623, R632, R624 OPTOISOLATORS
NEC | JC-2001VMA | FUZZY/DIM | ALIGNMENT
NEC | JC-1403 | YELLOW COLOR | COLD SOLDER ON CRT BOARD
NEC | JC-1403 | DEAD | CHECK FOR COLD SOLDER ON MAIN BOARD
NEC | JC-1531 | BAD PCC | C561 470/25V
NEC | JC-1531 | COLORS CHANGE RANDOMLY | COLD SOLDER AND C561 470/25V
NEC | JC-1531VMA | BRIGHT TO DIM…THEN DARK | CHECK FOR COLD SOLDER OR BAD CAPS ON VIDEO BOARD
NEC | JC-1402 | DEAD | IN PS: CHECK IC602 STK7404, R632, R624
NEC | JC-1402 | DEAD | R632, R624, R630, IC602, R615, TH601
NEC | JC-1733VMA | DEAD | CHECK PS: Q6C2, R6S8, 3842 IC'S
NEC | JC-1402 | FUZZY | BAD FLYBACK 47-105-647
NEC | JC-1404HMA | BAD COLORS | IC901, AND FLYBACK 420016-01
NEC | JC-1531 | FUZZY…NO RED | CLEAN RED INPUT CONNECTOR…ALIGN
NEC | JC-1401 | DEAD | IC302 STK7404, FUSE
NEC | JC-1403 | DEAD | COLD SOLDER ON P/S
NEC | JC-2001 | NO HORIZONTAL | TR504, TR508, F501 1A PICO
NEC | JC-1535VMA | BAD COLOR | VIDEO IC LM1203N, CHECK FOR LOCAL AREA COLD SOLDER
NEC | JC-2141VMA | 6FG, DEAD | BAD POWER SUPPLY SWITCH
NEC | JC-1403 | NO GREEN | REPLACE GREEN TRANSISTOR 2SC3953 ECG2501
NEC | JC1601 | DEAD | HOT BAD…2SC3688 AND CHECK Q5TO FOR SHORT
NEC | 3V | NO VIDEO OR DISTORTED | BAD LM1203 ON MAIN BOARD
NEC | JC1601 | DEAD, SHORTED HOT KEEPS BLOWING | REPLACE HOT AND CHECK Q5PO=K758 (REGULATOR FOR HOT B)