#

9.4 CD Mechanism Test (For error code F15, F26, F16, F17, F27, F28, F29, H15)

TOP PREVIOUS NEXT

1. Press “CD”.

2. Press “OPEN/CLOSE (1)” and place a CD.

3. Press “OPEN/CLOSE (1)” to close the tray.

4. Press “OPEN/CLOSE (5)” and wait until the tray is open.

5. Press “OPEN/CLOSE (1)” and remove the CD.

6. Press “OPEN/CLOSE (1)” to close the tray.

7. Press “/TUNE MODE” to indicate Error Code.

   - If several problem exist, error code will change each time when “/TUNE MODE” is pressed. (e.g. F15 → F26 → F16 ....etc).

TOP PREVIOUS NEXT