#

10.5.1 Setting Method

TOP PREVIOUS NEXT

Lock Mode A

With the power turned to On, set the SELECTOR to “DVD/CD”. The lock function works by presing the “POWER” button on either the main unit or the remote control while continously pressing on the”TuneMODE” button on the main unit. (When the locked condition is working, “LOCKED” will appear on the display for 3 seconds before commencement of disc playback.)

Lock Mode B

With the power turned to ON, set the SELECTOR to DVD/CD. The lock function works by pressing the “POWER” button on either the main unit or the remote control while continously pressing on the “/MEMORY” buttonon the main unit. (When the locked condition is working, “LOCKED” will appear on the display for 3 seconds before commencement of disc playback.)

When in Lock Mode B, only the sound quality operating buttons will work while the rest of the buttons will not work.

TOP PREVIOUS NEXT