#

9.3.1 Tray Lock Function

TOP PREVIOUS NEXT

- There are two tray lock functions

- Power on through the SELECTOR /DVD/CD. While holding down the [CD STOP] button on the main unit press the [POWER] button on the main unit or the remote control. Lock Mode A will be entered, [_ _ _ _LOCKED_ _] will be displayedfor 3 seconds, and the current disc will begin playing.

- Lock Mode A will disable the button below while turning the power on or off.

  [OPEN/CLOSE]

- When locked in Lock Mode A pressing the [POWER] button on the main unit or the remote control while holding down the [CD STOP] button on the main unit will display [_ _UNLOCKED_ _] and unlock the unit.

- Power on through the SELECTOR DVD/CD. While holding down the [CD PLAY] button on the main unit press the [POWER] button on the main unit or the remote control. Lock Mode B will be entered, [_ _ _LOCKED_ _] will be displayed for 3 seconds,and the current disc will begin playing.

- In Lock Mode B the button below, mainly selector and disc operation related items, will be disabled.

  Main Unit: [OPEN/CLOSE] [PAUSE] [STOP] [I<</V] [SELECTOR] [DISK SKIP]

  Remote Control: [AUX] [DVD/CD] [TV] [VCR] [TUNER/BAND] [0] ~ [9] [>=10] [DISK]

  [I<<] [I>>] [PAUSE] [STOP] [<<] [>>] [REPEAT] [POSITION]

  [A-B REPEAT] [MARKER] [DISPLAY] [MIX2ch] [TEST] [TIMER] [FL DISPLAY] [CH SELECT]

  [KARAOKE ON/OFF] [KARAOKE DISPLAY] [VOICE] [MUTE]

  [ECHO] [b] [#] [CENTER FOCUS] {SEAT POSITION] [RETURN] [DISK SKIP]

  [CINEMA] [GROUP] [PAGE]

  While playing it is not necessary to re-disable buttons disabled under Lock Mode B.

  Also, button related to sound quality are not disabled. The buttons below are not disabled.

  Main Unit: [POWER]

  Remote Control: [POWER] [DISK MANAGER] [PALY MODE] [CANCEL] [SFC] [SUBWOOFER LEVEL]

  [VOL-] [VOL+] [SUPER SURROUND] [DOLBY PROLOGIC] [SUB TITLE] [AUDIO] [ANGLE]

  [TOP MENU] [MENU] [ENTER] [<] [>] [^] [V] [MUTING] [PLAY]

- When locked in Lock Mode B pressing the [POWER] button on the main unit or the remote control while holding down the [CD PLAY] button on the main unit will unlock the unit after displaying [_ _UNLOCKED_ _] for 3 seconds.

- Tray lock is canceled when AC power is cut.

- Tray lock A and B functions are exclusive operations. The first one enabled will have priority.

- In Lock Mode A any selector button is allowed to start auto power on.

  In Lock Mode B all selector buttons are disable from starting auto power on.

- When a disabled button is pressed while in lock mode [_ _ _LOCKED_ _] will be displayed for 3 seconds on the front display panel.

- Lock mode will be cancelled when a loading error occurs with the CR20.

  (If the [OPEN/CLOSE] button were disabled when the tray is opened by a TAKE OUT DISC error recovery would be impossible)

TOP PREVIOUS NEXT