#

7.1 Checking for DVD B/E Module (1/2) and Power Switch P.C.B..

TOP PREVIOUS NEXT

Step 3 Slightly spread open both sides of the cabinet before lifting it upwards to remove.

- Carry out the check for DVD B/E Module (1/2) board, AC input board as per condition indicated in diagram below.

Step 6 Remove FFC from connector. (FP2001)

Step 7 Overturn DVD B/E Module (2/2) P.C.B..

Step 8 Connect back extension FFC to connector. (FP2001)

- Carry out check for DVD Module (2/2) board as per condition in diagram below.

[Caution] Lay thick paper below the board.

TOP PREVIOUS NEXT