#

Service Manual

TOP NEXT

ORDER NO. MD0203047C1

A6

DVD Home Theatre Sound System

- SA-HT67P

Colour

(S)... Silver Type

DVD/CD SECTION :

DL1 MECHANISM SERIES

Specifications
AMPLIFIER SECTION |
FTC TTL Power Output | 250 W
120 Hz-20 kHz, 1.0% total harmonic distortion
Front | 28 W per channel (6Ω)
Center | 28 W (6Ω)
Surround | 28 W per channel (6Ω)
45 Hz-120 Hz, 1.0% total harmonic distortion
Subwoofer | 110 W (6Ω)
RMS TTL Power Output | 350 W
1 kHz, 10% total harmonic distortion
Front | 38 W per channel (6Ω)
Center | 38 W (6Ω)
Surround | 38 W per channel (6Ω)
100 Hz, 10% total harmonic distortion
Subwoofer | 160 W (6Ω)
Input sensitivity/input impedance |
AUX | 250 mV, 10 kΩ
DISC SECTION |
Disc |
DVD | 8 cm (3”)/12 cm (5”) single-side, single-layer
| 8 cm (3”)/12 cm (5”) single-side, double-layer
| 8 cm (3”)/12 cm (5”) double-side, double-layer
| (One layer per side)
CD/ VCD | 8 cm (3”)/12 cm (5”) (CD-R/RW)
Video |
Signal system | NTSC
Output level | Composite video 1 Vp-p (75Ω)
S-video Y | 1 Vp-p (75Ω)
S-video C | 0.286 Vp-p (75Ω/NTSC)
Audio |
Sampling frequency |
CD | 44.1 kHz
DVD | 48 kHz/96 kHz
Decoding | 16/20/24 bit linear
Wow and flutter | Below measurable limit
D/A converter | Delta-sigma DAC
Pick up |
Beam Source | Semiconductor Laser
Wavelength |
DVD | 658 nm
VCD/CD | 790 nm
FM TUNER SECTION |
Frequency range | 87.9-107.9 MHz (200 kHz steps)
| 87.5-108.0 MHz (100 MHz steps)
Sensitivity | 16.0 dBf (1.7μV, IHF)
Antenna Terminals | 75Ω unbalanced
AM TUNER SECTION |
Frequency range | 520 - 1710 kHz (10 kHz steps)
Sensitivity |
S/N 20 dB at 1000 kHz | 600μV/m
GENERAL |
Power supply | AC 120 V, 60 Hz
Power consumption | 190 W
Power consumption in standby mode
| 0.25 W
Dimensions (W x H x D) | 430 x 114 x 368 mm
| (16 15/16”x4 1/2”x14 1/2”)
Mass | 8.4 kg(18.5 Ib.)
SYSTEM |
SC-HT67 (P) | Main unit: SA-HT67 (P)
| Speaker unit: SB-HT75 (P)
Subwoofer: SB-W95 (P)
Notes: Specifications are subject to change without notice. Weight and dimensions are approximate. Total harmonic distortion is measured by the digital spectrum analyzer.

© 2002 Matsushita Electronics (S) Pte. Ltd. All rights reserved. Unauthorized copying and distribution is a violation of law.

TOP NEXT