<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-PM11</Model>
<System>ORDER NO. MD0102023C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1301000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=May year=2001>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-PM11</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>13.1 IC701 (AN8885NSBE1) Servo Amplifier</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1300000000x
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1302000000
</nmlist>
</nameloc>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.624in"><colspec colnum="2" colname="2" colwidth="0.578in"><colspec colnum="3" colname="3" colwidth="0.417in"><colspec colnum="4" colname="4" colwidth="1.779in"><thead><row rowsep="1"><entry colname="1" align="center"><Para><emphasis>Pin No.</emphasis>
</Para>
</entry>
<entry colname="2" align="center"><Para><emphasis>Mark</emphasis>
</Para>
</entry>
<entry colname="3" align="center"><Para><emphasis>I&sol;O</emphasis>
</Para>
</entry>
<entry colname="4" align="center"><Para><emphasis>Function</emphasis>
</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>PDE</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tracking signal input 1</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>PDF</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tracking signal input 2</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>3</Para>
</entry>
<entry colname="2" align="justify"><Para>VCC</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Power supply</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>PDA</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Focus signal input terminal 1</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>PDB</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Focus signal input terminal 2</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>6</Para>
</entry>
<entry colname="2" align="justify"><Para>LPD</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>APC amp input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>7</Para>
</entry>
<entry colname="2" align="justify"><Para>LD</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>APC amp output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>8</Para>
</entry>
<entry colname="2" align="justify"><Para>RF</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>RFsumming output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>9</Para>
</entry>
<entry colname="2" align="justify"><Para>RFIN</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Detector&rsquo;s input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>10</Para>
</entry>
<entry colname="2" align="justify"><Para>CSBRT</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Capacitor for OFTR connection</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>11</Para>
</entry>
<entry colname="2" align="justify"><Para>CEA</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Capacitor for HPF amp connection</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>12</Para>
</entry>
<entry colname="2" align="justify"><Para>BDO</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>BDO output (&ldquo;H&rdquo; : drop out)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>13</Para>
</entry>
<entry colname="2" align="justify"><Para>LDON</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>APC control</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>14</Para>
</entry>
<entry colname="2" align="justify"><Para>GND</Para>
</entry>
<entry colname="3" align="justify"><Para>&mdash; </Para>
</entry>
<entry colname="4" align="justify"><Para>Ground</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>15</Para>
</entry>
<entry colname="2" align="justify"><Para>&sol;RFDET</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>NRFDET output (&ldquo;L&rdquo; : detection)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>16</Para>
</entry>
<entry colname="2" align="justify"><Para>PDOWN</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Power-down input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>17</Para>
</entry>
<entry colname="2" align="justify"><Para>OFTR</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>OFTR output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>18</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>N.C.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>19</Para>
</entry>
<entry colname="2" align="justify"><Para>ENV</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>3T-ENV output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>20</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>N.C.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>21</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>N.C.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>22</Para>
</entry>
<entry colname="2" align="justify"><Para>TEN</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>TE amp input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>23</Para>
</entry>
<entry colname="2" align="justify"><Para>TEOUT</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>TE amp output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>24</Para>
</entry>
<entry colname="2" align="justify"><Para>FEOUT</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>FE amp output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>25</Para>
</entry>
<entry colname="2" align="justify"><Para>FEN</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>FE amp input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>26</Para>
</entry>
<entry colname="2" align="justify"><Para>VREF</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Reference voltage output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>27</Para>
</entry>
<entry colname="2" align="justify"><Para>TBAL</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tracking balance control</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>28</Para>
</entry>
<entry colname="2" align="justify"><Para>FBAL</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Focus balance control</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1300000000x
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1302000000
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
